| **A. ROAD TEST** |  | **C. EXTERIOR** |  | **E. FRONT AXLE** |  |
| --- | --- | --- | --- | --- | --- |
| STARTER ACTION |   | BODY DAMAGE |   | FLUID LEAKS |  |
| ENGINE OPERATION |   | HOOD AND FENDERS |   | STEERING LINKAGE |  |
| OIL PRESSURE |   | STIRRUP STEPS |   | SHOCK ABSORBERS |  |
| HORNS  |   | LICENSE PLATES |   | BRAKE LINING |  |
| LIGHTS-WARNING /BUZZERS |   | TOW HOOKS |   | SLACK ADJUSTERS |  |
| CLUTCH |   | BUMPERS |   | SPRINGS |  |
| STEERING |   | ALL TIRES AND WHEELS |   | KING PINS & BUSHINGS |  |
| TRANSMISSION |   | ALL LIGHTS & SIGNALS |   | WHEEL CYLINDER/CALIPER |  |
| BACK-UP ALARM |   | REFELCTORS |   | HUB, DRUMS, ROTORS |  |
| BRAKE CHECK |   | RETROREFLECTIVE TAPE |   | WHEEL BEARINGS |  |
| INSTRUMENTATION |   | PAINT AND LETTERING |   | WHEEL BALANCE |  |
| MIRRORS |   | MIRRORS |   | ALIGNMENT |  |
| HEATER/DEFROSTER |   | STORAGE & CHAIN BOXES |   | **F. REAR AXLE** |  |
| WINDSHIELD WIPERS |   | **D. ENGINE COMPARTMENT** |  | FLUID LEAKS |  |
| WINDSHIELD WASHERS |   | ALL BELTS |  | AXLE VENTS |  |
| STOP ARM/XING GUARD |   | LEAKS |  | SHOCK ABSORBERS |  |
| GOVERNOR |   | GOVERNOR(S) |  | BRAKE LINING |  |
| **B. BODY INTERIOR** |   | FAN ASSEMBLY |   | SLACK ADJUSTERS |  |
| AISLE AND FLOOR |  | WATER PUMP |   | SPRINGS  |  |
| INTERIOR PANELS |  | AIR COMPRESSOR |   | KING PINS & BUSHINGS |  |
| ENTRANCE DOOR |  | ALL PIPING & HOSES |   | WHEEL CYLINDER/CALIPER |  |
| EMERGENCY DOOR & EXITS |   | ALL WIRING |   | HUB, DRUMS, ROTORS |  |
| EMERGENCY EQUIPMENT |   | STEERING GEAR  |   | WHEEL BEARINGS |  |
| DRIVER’S SEAT |   | HYDRALIC PUMP |   | WHEEL BALANCE |  |
| STEPS  |   | MASTER CYLINDER |   | WHEEL SEALS |  |
| PASSENGER SEATS & BELTS |   | BRAKE BOOSTER |   | **G. UNDER BUS** |  |
| STANCHISONS /BARRIERS |   | RADIATOR MOUNTING |   | EXHAUST SYSTEM |  |
| SUNSHIELD/VISOR |   | FUEL SYSTEM |   | CLUTCH |  |
| ALL GLASS / WINDOWS  |   | BATTERY(S) |   | AIR TANKS |  |
| LIFT OR RAMP  |   | CRANKCASE VENT VALVE |  | TRANSMISSION |  |
| WHEELCHAIR POSITIONS |   | TURBOCHARGER |  | PARKING BRAKE |  |
| RADIOS AND CAMERAS |   | VIBRATION DAMPER |  | DRIVE LINE |  |
| INTERIOR WIRING |   | ENGINE MOUNTS |  | FUEL TANK & FUEL LINES |  |
| ALL OPENINGS |   | COOLING SYSTEM |  | HOSE-PIPING-WIRING |  |
| STORAGE COMPARTMENTS |   |  |  | AIR DRYER |  |
| POSTERS AND STICKERS |   |  |  | BRAKE CHAMBERS |  |
| LOOSE OBJECTS & CLEANLINESS |   |  |  | FRAME & CROSSMEMBER |  |
| Comments: |  |  |  |
| HANDRAILS |   |  |  |  |  |
|  |   |  |
|  |   |
|  |   |

R

 For Printing Purposes only

Rev. 2/18 **VIRGINIA DEPARTMENT OF EDUCATION**

BUS INSPECTION: EVERY 45 SCHOOL DAYS OR 5000 MILES

DATE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_MILEAGE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_BUS #\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_CHASIS#\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

INDICATE THE CONDITION OF EACH ITEM IS THE SPACE PROVIDED WITH THE FOLLOWING:

( / ) = OK (A) = ADJUSTMENT MADE (X) = REPAIR MADE (N) = REPAIR NEEDED (O) OUT OF SERVICE

MECHANIC or INSPECTOR\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_DATE COMPLETED\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_