| **A. ROAD TEST** |  | **C. EXTERIOR** |  | **E. FRONT AXLE** |  |
| --- | --- | --- | --- | --- | --- |
| STARTER ACTION |  | BODY DAMAGE |  | FLUID LEAKS |  |
| ENGINE OPERATION |  | HOOD AND FENDERS |  | STEERING LINKAGE |  |
| OIL PRESSURE |  | STIRRUP STEPS |  | SHOCK ABSORBERS |  |
| HORNS |  | LICENSE PLATES |  | BRAKE LINING |  |
| LIGHTS-WARNING /BUZZERS |  | TOW HOOKS |  | SLACK ADJUSTERS |  |
| CLUTCH |  | BUMPERS |  | SPRINGS |  |
| STEERING |  | ALL TIRES AND WHEELS |  | KING PINS & BUSHINGS |  |
| TRANSMISSION |  | ALL LIGHTS & SIGNALS |  | WHEEL CYLINDER/CALIPER |  |
| BACK-UP ALARM |  | REFELCTORS |  | HUB, DRUMS, ROTORS |  |
| BRAKE CHECK |  | RETROREFLECTIVE TAPE |  | WHEEL BEARINGS |  |
| INSTRUMENTATION |  | PAINT AND LETTERING |  | WHEEL BALANCE |  |
| MIRRORS |  | MIRRORS |  | ALIGNMENT |  |
| HEATER/DEFROSTER |  | STORAGE & CHAIN BOXES |  | **F. REAR AXLE** |  |
| WINDSHIELD WIPERS |  | **D. ENGINE COMPARTMENT** |  | FLUID LEAKS |  |
| WINDSHIELD WASHERS |  | ALL BELTS |  | AXLE VENTS |  |
| STOP ARM/XING GUARD |  | LEAKS |  | SHOCK ABSORBERS |  |
| GOVERNOR |  | GOVERNOR(S) |  | BRAKE LINING |  |
| **B. BODY INTERIOR** |  | FAN ASSEMBLY |  | SLACK ADJUSTERS |  |
| AISLE AND FLOOR |  | WATER PUMP |  | SPRINGS |  |
| INTERIOR PANELS |  | AIR COMPRESSOR |  | KING PINS & BUSHINGS |  |
| ENTRANCE DOOR |  | ALL PIPING & HOSES |  | WHEEL CYLINDER/CALIPER |  |
| EMERGENCY DOOR & EXITS |  | ALL WIRING |  | HUB, DRUMS, ROTORS |  |
| EMERGENCY EQUIPMENT |  | STEERING GEAR |  | WHEEL BEARINGS |  |
| DRIVER’S SEAT |  | HYDRALIC PUMP |  | WHEEL BALANCE |  |
| STEPS |  | MASTER CYLINDER |  | WHEEL SEALS |  |
| PASSENGER SEATS & BELTS |  | BRAKE BOOSTER |  | **G. UNDER BUS** |  |
| STANCHISONS /BARRIERS |  | RADIATOR MOUNTING |  | EXHAUST SYSTEM |  |
| SUNSHIELD/VISOR |  | FUEL SYSTEM |  | CLUTCH |  |
| ALL GLASS / WINDOWS |  | BATTERY(S) |  | AIR TANKS |  |
| LIFT OR RAMP |  | CRANKCASE VENT VALVE |  | TRANSMISSION |  |
| WHEELCHAIR POSITIONS |  | TURBOCHARGER |  | PARKING BRAKE |  |
| RADIOS AND CAMERAS |  | VIBRATION DAMPER |  | DRIVE LINE |  |
| INTERIOR WIRING |  | ENGINE MOUNTS |  | FUEL TANK & FUEL LINES |  |
| ALL OPENINGS |  | COOLING SYSTEM |  | HOSE-PIPING-WIRING |  |
| STORAGE COMPARTMENTS |  |  |  | AIR DRYER |  |
| POSTERS AND STICKERS |  |  |  | BRAKE CHAMBERS |  |
| LOOSE OBJECTS & CLEANLINESS |  |  |  | FRAME & CROSSMEMBER |  |
| Comments: |  |  |  |
| HANDRAILS |  |  |  |  |  |
|  |  |  | | | |
|  |  |
|  |  |

R

For Printing Purposes only

Rev. 2/18 **VIRGINIA DEPARTMENT OF EDUCATION**

BUS INSPECTION: EVERY 45 SCHOOL DAYS OR 5000 MILES

DATE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_MILEAGE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_BUS #\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_CHASIS#\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

INDICATE THE CONDITION OF EACH ITEM IS THE SPACE PROVIDED WITH THE FOLLOWING:

( / ) = OK (A) = ADJUSTMENT MADE (X) = REPAIR MADE (N) = REPAIR NEEDED (O) OUT OF SERVICE

MECHANIC or INSPECTOR\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_DATE COMPLETED\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_